Retevis CPS V1.2.8 Changelog
1、Add RX/TX Display setting, you can select to show the channel name, frequency or RSSI on the RX/TX window on HA1G/HA1UV.
2、Allowed to program air band channel via the CPS on HA1G/HA1UV.
